S7 RHOMBOS EXTERIOR | Exterior ceiling rail channel system


	Pos ...............
............... m²
	Delivery and installation of durlum expanded metal panels of the S7 RHOMBOS EXTERIOR V1 system.

A frame is butt welded onto the cut-to-size expanded metal panels. By this, exact fitting parts are produced. The expanded metal panels are hung in a positive locking and tension-free way into a special substructure [see separate position], then secured with a special concealed ball impact-resistant feature U2053 WS. 

Tolerances and quality requirement according to the durlum standard.

Material:	steel with special treatment, suitable for outdoor use
Variant:	V1 [surface-welded frame]
Mesh.	M260_1.5
Mesh length:	28 mm
Mesh width:	12 mm
Web width:	2.0 mm
Web thickness:	1.5 mm 
Exp. metal thickness:	approx. 3.6 mm
Surface:	powder-coated RAL 9016 matt [alternative RAL ...............]
Layer thickness:	approx. 60 µm
Dimension:	length: ............... mm
	width: ............... mm
€ / m²

	
	

	Pos ...............
	Set-up costs depending on format, design and call-up.
€

	
	

	Pos ...............
............... m²
	Delivery and installation of a durlum S7 RHOMBOS EXTERIOR substructure system, 

consisting of aluminium carrier profile W2053, bolted with M12 screws and nuts to AFH-661 suspension brackets. The suspension brackets are suspended from the structural ceiling by threaded rods. 
The longitudinal connection of the carrier profiles is made using carrier longitudinal connectors W2053-V. Connection to walls is made using wall anchors U1042. 
For transverse bracing, perforated L-shaped carrier U1040 are connected to the W2053 profiles using U1045 module adapters. 
The U1040 must be connected at longitudinal joints using U1041 longitudinal connectors [bolted connection]. 
The spacing of the transverse bracing shall be designed in accordance with DIN EN 13964 and the installation instructions and must be verified and defined by the contractor. 
The spacing of the carrier profiles must be matched exactly to the width of the expanded metal panels so that the panels can be installed without stress. Care must be taken to ensure level and aligned installation. 
Only structural components approved by the manufacturer of the expanded metal panels may be used. All parts are made of aluminium/galvanized steel sheet. 

Surface of the rail channels:	black, optionally painted to RAL ...............
Layer thickness:	approx. 60 µm
Suspension height:	............... mm
€ / m²

	
	

	Pos ...............
............... running metre
	Delivery and installation of durlum wall connection profiles made of steel.

Surface:	powder-coated RAL 9016 matt [alternative RAL ...............]
Profile form:	U profile
€/running metre



